Répertoire national de l’Offre et des Ressources en santé et accompagnement médico-social
0.5.0-snapshot-1 - ci-build

Répertoire national de l’Offre et des Ressources en santé et accompagnement médico-social - Local Development build (v0.5.0-snapshot-1) built by the FHIR (HL7® FHIR® Standard) Build Tools. See the Directory of published versions

## Resource Profile: RORLocation - Mappings

Draft as of 2025-02-17

Mappings for the ror-location resource profile.

### Mappings for Location du Modèle exposition ROR V3 ()

RORLocation
Location | LieuRealisationOffre |
id | metadonnee.identifiant |
meta | metadonnee |
lastUpdated | dateMiseJour |
tag (codeRegion) | regionSource |
identifier (idExterneSynchro) | idExterneSynchro | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
identifier (idLocation) | identifiant | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
status | Pas d'équivalent |
operationalStatus | Statut | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
name | nom | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
alias (nomExterneSynchro) | nomExterneSynchro |
description | description | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
type | fonctionLieu | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
telecom | telecommunication | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 si champ d'activité = MS ou AMBULATOIRE (sauf si uniteSensible = Oui), Profil 0 si champ d'activité = AMBULATOIRE (sauf si uniteSensible = Oui)
value | adresseTelecom | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 si champ d'activité = MS ou AMBULATOIRE (sauf si uniteSensible = Oui), Profil 0 si champ d'activité = AMBULATOIRE (sauf si uniteSensible = Oui)
address | adresse | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
line |  |
extension (careOf) | pointRemise | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
extension (additionalLocator) | complementPointGeographique | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
extension (houseNumber) | numeroVoie | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
extension (buildingNumberSuffix) | extension | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
extension (streetNameType) | typeVoie | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
extension (streetNameBase) | libelleVoie | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
extension (postalBox) | mentionDistribution | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
extension (lieuDit) | lieuDit | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
city | localite | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
postalCode | codePostal | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
position | coordonneeGeographique | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
longitude | longitude | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)
latitude | latitude | Profil 1, Profil 2 (sauf si uniteSensible = Oui), Profil 3 (sauf si uniteSensible = Oui), Profil 0 (sauf si uniteSensible = Oui)

### Mappings for RIM Mapping (http://hl7.org/v3)

RORLocation
Location | Entity. Role, or Act, .Role[classCode=SDLC]
meta | n/a, N/A
id | n/a
extension | n/a, N/A
versionId | n/a
lastUpdated | n/a
source | n/a
profile | n/a
security | n/a, CV
tag | n/a, CV
tag (codeRegion) | n/a, CV
implicitRules | n/a
language | n/a
text | n/a, N/A, Act.text?
contained | Entity. Role, or Act, N/A
modifierExtension | n/a, N/A
identifier | n/a, II - The Identifier class is a little looser than the v3 type II because it allows URIs as well as registered OIDs or GUIDs. Also maps to Role[classCode=IDENT], .id
identifier (idExterneSynchro) | n/a, II - The Identifier class is a little looser than the v3 type II because it allows URIs as well as registered OIDs or GUIDs. Also maps to Role[classCode=IDENT], .id
id | n/a
extension | n/a, N/A
use | n/a, Role.code or implied by context
type | n/a, CD, Role.code or implied by context
id | n/a
extension | n/a, N/A
coding | n/a, CV, union(., ./translation)
id | n/a
extension | n/a, N/A
system | n/a, ./codeSystem
version | n/a, ./codeSystemVersion
code | n/a, ./code
display | n/a, CV.displayName
userSelected | n/a, CD.codingRationale
text | n/a, ./originalText[mediaType/code="text/plain"]/data
system | n/a, II.root or Role.id.root
value | n/a, II.extension or II.root if system indicates OID or GUID (Or Role.id.extension or root)
period | n/a, IVL<TS>[lowClosed="true" and highClosed="true"] or URG<TS>[lowClosed="true" and highClosed="true"], Role.effectiveTime or implied by context
assigner | n/a, The target of a resource reference is a RIM entry point (Act, Role, or Entity), II.assigningAuthorityName but note that this is an improper use by the definition of the field. Also Role.scoper
identifier (idLocation) | n/a, II - The Identifier class is a little looser than the v3 type II because it allows URIs as well as registered OIDs or GUIDs. Also maps to Role[classCode=IDENT], .id
id | n/a
extension | n/a, N/A
use | n/a, Role.code or implied by context
type | n/a, CD, Role.code or implied by context
id | n/a
extension | n/a, N/A
coding | n/a, CV, union(., ./translation)
id | n/a
extension | n/a, N/A
system | n/a, ./codeSystem
version | n/a, ./codeSystemVersion
code | n/a, ./code
display | n/a, CV.displayName
userSelected | n/a, CD.codingRationale
text | n/a, ./originalText[mediaType/code="text/plain"]/data
system | n/a, II.root or Role.id.root
value | n/a, II.extension or II.root if system indicates OID or GUID (Or Role.id.extension or root)
period | n/a, IVL<TS>[lowClosed="true" and highClosed="true"] or URG<TS>[lowClosed="true" and highClosed="true"], Role.effectiveTime or implied by context
assigner | n/a, The target of a resource reference is a RIM entry point (Act, Role, or Entity), II.assigningAuthorityName but note that this is an improper use by the definition of the field. Also Role.scoper
status | n/a, .statusCode
operationalStatus | n/a, CV
name | n/a, .name
alias | n/a, .name
alias (nomExterneSynchro) | n/a, .name
description | n/a, .playingEntity[classCode=PLC determinerCode=INSTANCE].desc
mode | n/a, .playingEntity[classCode=PLC].determinerCode
type | n/a, CD, .code
telecom | n/a, TEL, .telecom
id | n/a
system | n/a, ./scheme
value | n/a, ./url
use | n/a, unique(./use)
rank | n/a
period | n/a, IVL<TS>[lowClosed="true" and highClosed="true"] or URG<TS>[lowClosed="true" and highClosed="true"], ./usablePeriod[type="IVL<TS>"]
address | n/a, AD, .addr
id | n/a
extension | n/a, N/A
use | n/a, unique(./use)
type | n/a, unique(./use)
text | n/a, ./formatted
line | n/a, AD.part[parttype = AL]
id | n/a
extension | n/a, N/A
extension (careOf) | ADXP[partType=CAR]
extension (additionalLocator) | ADXP[partType=ADL]
extension (houseNumber) | ADXP[partType=BNR]
extension (buildingNumberSuffix) | ADXP[partType=BNS]
extension (streetNameType) | ADXP[partType=STTYP]
id | n/a
url | N/A
value[x] | N/A
extension (streetNameBase) | ADXP[partType=STB]
extension (postalBox) | ADXP[partType=POB]
city | n/a, AD.part[parttype = CTY]
district | n/a, AD.part[parttype = CNT | CPA]
state | n/a, AD.part[parttype = STA]
postalCode | n/a, AD.part[parttype = ZIP]
country | n/a, AD.part[parttype = CNT]
period | n/a, IVL<TS>[lowClosed="true" and highClosed="true"] or URG<TS>[lowClosed="true" and highClosed="true"], ./usablePeriod[type="IVL<TS>"]
physicalType | n/a, CD, .playingEntity [classCode=PLC].code
position | n/a, .playingEntity [classCode=PLC determinerCode=INSTANCE].positionText
id | n/a
extension | n/a, N/A
modifierExtension | n/a, N/A
longitude | n/a, (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
latitude | n/a, (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
altitude | n/a, (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
managingOrganization | n/a, The target of a resource reference is a RIM entry point (Act, Role, or Entity), .scopingEntity[classCode=ORG determinerKind=INSTANCE]
partOf | n/a, The target of a resource reference is a RIM entry point (Act, Role, or Entity), .inboundLink[typeCode=PART].source[classCode=SDLC]
hoursOfOperation | n/a, .effectiveTime
id | n/a
extension | n/a, N/A
modifierExtension | n/a, N/A
daysOfWeek | n/a, .effectiveTime
allDay | n/a, .effectiveTime
openingTime | n/a, .effectiveTime
closingTime | n/a, .effectiveTime
availabilityExceptions | n/a
endpoint | n/a, The target of a resource reference is a RIM entry point (Act, Role, or Entity)

### Mappings for FiveWs Pattern Mapping (http://hl7.org/fhir/fivews)

RORLocation
Location |
identifier | FiveWs.identifier
identifier (idExterneSynchro) | FiveWs.identifier
identifier (idLocation) | FiveWs.identifier
status | FiveWs.status
operationalStatus | FiveWs.status
mode | FiveWs.class
type | FiveWs.class
physicalType | FiveWs.class