Guide d'implémentation FHIR - Mesures de santé
3.1.0 - ci-build

Guide d'implémentation FHIR - Mesures de santé - Local Development build (v3.1.0) built by the FHIR (HL7® FHIR® Standard) Build Tools. See the Directory of published versions

## Example Device: phd-74E8FFFEFF051C00

Profil: PhdDevice

identifier: IEEE 11073 System Identifier/74-E8-FF-FE-FF-05-1C-00, Bluetooth MAC address/00-1C-05-FF-E8-74

manufacturer: Nonin_Medical_Inc.

serialNumber: 501900083

modelNumber: Model 3230

type: MDC_MOC_VMS_MDS_SIMP

### Specializations

- | SystemType | Version
* | MDC_DEV_SPEC_PROFILE_PULS_OXIM: Pulse Oximeter | 1

> version

> type: MDC_ID_PROD_SPEC_FW: Firmware revision

> value: r2.1

> version

> type: MDC_ID_PROD_SPEC_SW: Software revision

> value: r1.5 9.7

> version

> type: MDC_ID_PROD_SPEC_HW: Hardware revision

> value: r1.0

> version

> type: MDC_REG_CERT_DATA_CONTINUA_VERSION: Continua version

> value: 6.0

> property

> type: MDC_REG_CERT_DATA_CONTINUA_CERT_DEV_LIST: certified device list as transport-specialization combo

> valueCode: BTLE Pulse Oximeter certified

> property

> type: regulation-status

> valueCode: Device is Regulated

> property

> type: MDC_TIME_SYNC_PROTOCOL: Time synchronization protocol

> valueCode: MDC_TIME_SYNC_NONE: